**Lab 2A: General-purpose input/output (GPIO) and serial communication**

**1. Open a Terminal on macOS/Linux or**[**Git Bash**](https://gitforwindows.org/)**on Windows, and make sure Serial Council is disabled**

**2. Serial**[**loopback**](https://en.wikipedia.org/wiki/Loopback)**test**

* Connect two serial pins (the 4th and 5th pins from the left of the top row) using one DuPont female-to-female [jump wires](https://en.wikipedia.org/wiki/Jump_wire)
* Install and run [Minicom](https://en.wikipedia.org/wiki/Minicom)

